**Desription:**

* Blink leds sequentially based on RTOS scheduler.

**Config:**

* Use user leds connected to the I/O PD13 and PD12 of the STM32F407VGT6.

A close-up of a green and black push pins

Description automatically generated

* Setup FreeRTOS config

A screenshot of a software pack

Description automatically generated

A screenshot of a computer

Description automatically generated

* Create tasks:

A screenshot of a computer program

Description automatically generated

**Debug with SWV to test this program**

More detail at README.md

A screenshot of a computer

Description automatically generated