**Desription:**

* Toggle led by periodically.

**Config:**

* Use user LD3 connected to the I/O PD13 of the STM32F407VGT6.

