**Desription:**

* Toggle led by pressing button, use button as external interrupt.

**Config:**

* In main.c:

A close-up of a computer code

AI-generated content may be incorrect.

* + choose any user led from LD3 -> LD6
  + choose port, pin for your button (e.g. I use built-in button)