
**Desription:**


* Blinking led using ODR register.

**Config:**

* In main.c:



* + choose any user led from LD3 -> LD6
  + stuff any value for period of blinking
* In Led.h:



* + choose ODR or BSRR register to set bit for blinking led