**Desription:**

* Adjust the brightness of led.

**Config:**

* Config clock source and PWM mode:

A screenshot of a computer

Description automatically generated

**Connection:**

* Use PE9 pin as PWM channel

A screen shot of a computer

Description automatically generated

* Connect PE9 to anode of led (use resistor < 1k ohm).
* Connect GND to cathode of led.